updating BIOS on B1/B3/C1/C3/IDS touchcomputers:

1. Create a bootable usb jump drive using the HP Disk format utility that was included with download that was sent. All necessary files for creating the bootable drive are included in the BIOSUPDATE.ZIP file. 

2. After creating the bootable jump drive, copy all of the BIOS update files from the BIOSUPDATE.ZIP file, to the USB jump stick. 

3. Insert the USB jump stick in a USB port on the B1/B3/C1/C3/IDS touchcomputer and boot up following the B1_B3_C3_IDS_BIOS Update Procedure.pdf. 