|  |  |
| --- | --- |
| cid:image004.png@01D1FD62.7E14CDD0 | **REVISION HISTORY** |

**REVISION HISTORY**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Configuration Files Rev** | **Elo released document number & revision** | **ECO Number** | **Date** | **Author** | **Description** |
| V07\_T1 | PCFG0056 Rev A | CO-19-1294 | JUL 18, 2019 | Kurtis Yang | * Initial release |
| V09 | PCFG0056 Rev B | CO-20-0191 | JAN 07, 2020 | Kurtis Yang | * Fix wake on touch problem, Disable A\_epn function when system in to sleep mode. * Increase touch accuracy. * Change ID=5 to ID=2 to fix water line saturation issue. * Fix CS 3V test fail at Elo Taipei office * Enhance AFE gain, increase SNR, and improve IC background noise issue. |